

JU-DK0C11-S1 - FW Update Instructions


The update tool runs in Windows PC only

1. Connect the Thunderbolt Dock to the Windows PC.
2. Double click the “EHDDPV\_DP\_FW\_Update.exe” (Need to run as administrator).
3. Connect your DP monitor to the DP port located next to the AC power jack.




1. The FW update procedure will run automatically, you can check the DP FW version before updating.






1. After the updating procedure completes, please unplug the AC Power and wait at least 10 seconds, then re-plug in the AC Power and wait for Thunderbolt Dock to power-on. Then press any key to continue.



1. You can confirm the DP FW version after completing the FW Update procedure.



Troubleshooting:

1. If DP firmware version doesn’t show, please check that the DP monitor is connected to the port next to the AC adapter jack.