- Video Switching
- Video Wall

- HDMI Audio Routing
- Analog Audio Routing

- RS-232 Routing
- Infrared Routing

- Firmware Update
- Backup and Restore
- System Logs

- Video Routing
- HDMI Audio Routing
- Analog Audio Routing
- RS-232 Routing
- Infrared Routing

Connect to Server Connect
Decoders
+

- All

- All Displays All_Rx

Encoders
+

- All

Parameters
Save to Preset
Wall Size
Wall Dreg Here To Use Wall Wall Monitors 1920x1080
Bezel Top
Bezel Bottom
Bezel Left
Bezel Right
Wall Decoders
Decoders
+

- All

- All Displays All_Rx

Encoders
+

- All

Preset X
Save Recall
Video Wall X
Must be a number between 1 and 5!
OK
Decoders
+

- All

- All Displays All_Rx

Encoders
+

- All

Decoders
+

- All

- All Displays All_Rx

Encoders
+

- All

Receivers
+

- All

- All Receivers All_Rx
- All Server API

Senders
+

- All

Receivers
+

- All

- All Receivers All_Rx
- All Server API

Senders
+

- All

Decoders
Reflesh

- All Device All

Create a Backup File
Save to Browse...
Restore From Device
Backup Location Select File Browse...
Rename X
Backup Successfully
OK
Decoders

- Type
  Date and Time
  Event ID
  User
  Details

Save to File Clean Log
Video Routing Table

- Encode
  Decode

Video Routing Table

- Encode
  Decode

Rename X
Confirm
New Device Wizard X
What type configuration do you want?
Default
Create a device with custom IP.
Custom
Create a device with advanced options.
Next>
Type in MAC Address X
Finish
Decoder Configuration X

- Analog Audio Output
- HDMI Audio Output
- Display EDID
- Network Setting
- RS232
- Tile Info

Audio Source
HDMI Audio(Downmix)
Analog Audio
Audio Source
HDMI Audio(from HDMI Video in Genlock)
Analog Audio
HDMI Audio(Stereo Downmix)
HDMI Audio(All Available Channels)
EDID
Hostname
IP Mode
IP Address
Subnet Mask
Default Gateway
Baud Rate
Data Bit
Stop Bit
Parity
Hostname
MAC Address
IP Address
Firmware
Current Video Mode(RX Video)
Multicast Streaming Address
Streaming Status
Video Resolution(Video)
Color Space(Video)
Tile info is not applies to firmware page
Save
Encoder Configuration X

- Input Setting
- Device EDID
- Network Setting
- RS232
- Tile Info

Input
HDCP Support
Save
HDCP 2.2 Support
Save
EDID
Save to Device Load from File
Hostname
IP Mode
IP Address
Subnet Mask
Default Gateway
Save
Baud Rate
Data Bit
Stop Bit
Parity
Save
Hostname
MAC Address
IP Address
Firmware
Multicast Streaming Address
Streaming Status
Video Resolution(Video)
Color Space(Video)
Save Tile info is not applies to firmware page
Selete X
Confirm