IPA System Manager
Version 1.0.1
VIDEO

- VIDEO SWITCHING
- VIDEO WALL

AUDIO

- HDMI AUDIO ROUTING
- ANALOG AUDIO ROUTING

INFRARED & RS-232

- RS-232 ROUTING
- INFRARED ROUTING

SYSTEM MANAGEMENT

- FIRMWARE UPDATE
- BACKUP AND RESTORE
- SECURITY
- SYSTEM LOGS

ROUTING TABLE

- VIDEO ROUTING
- HDMI AUDIO ROUTING
- ANALOG AUDIO ROUTING
- RS-232 ROUTING
- INFRARED ROUTING

CONNECT TO SERVER:
IP:
. . .
Port: CONNECT
Receiver (RX)
Preset:
Preset #1

- All Displays
  All

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  11
- Preset #2
  12
- Preset #3
  13
- Preset #4
  14
- Preset #5
  15
- Preset #6
  16
- Preset #7
  17
- Preset #8
  18
- Preset #9
  19

SET VIDEO MODE
Genlock
Genlock Scaling
Fast Switch Full Screen
SET VIDEO
Leave Video Channel
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Video Formats
HD720P
HD1080P
4K UHD 2160P
Cinema Formats
4K Cinema 4096x2160
Graphics Formats
1024x768P
1280x768
1280x960
1280x1024
1360x768
1400x1050
1600x1200
1680x1050
1920x1200
Set Framebuffer Mode
Keep Aspect Ratio
Stretch to Fit
Crop to Fit
Video Formats
HD 720P 50Hz
HD 720P 60Hz
HD 1080P 50Hz
HD 1080P 60Hz
4K UHD 2160P 25Hz
4K UHD 2160P 30Hz
4K UHD 2160P 50Hz
4K UHD 2160P 60Hz
Cinema Formats
4K Cinema 4096x2160 24Hz
4K Cinema 4096x2160 30Hz
4K Cinema 4096x2160 60Hz
Video Formats
1024x768 60Hz
1280x768 60Hz
1280x960 60Hz
1280x1024 60Hz
1360x768 60Hz
1400x1050 60Hz
1600x1200 60Hz
1680x1050 60Hz
1920x1200 60Hz
SET VIDEO MODE
Start Video
Stop Video
Stop and Free Multicast address
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Parameters
Wall Receiver (RX)
Bezel adjustment:
Top: px
Bottom: px
Left: px
Right: px
Preset #1
PRESET OPTIONS
Rename
Y N
Wall Size:
X: Y:

- Preset #1
  61
- Preset #2
  62
- Preset #3
  63
- Preset #4
  64
- Preset #5
  65
- Preset #6
  66
- Preset #7
  67
- Preset #8
  68
- Preset #9
  69

Y N

WALL FUNCTIONS
Wall Monitors Resolutions
VIDEO FORMATS
HD720P
HD1080P
4K UHD
CINEMA FORMATS
4K Cinema 4096x2160
GRAPHICS FORMATS
1024x768
1280x768
1280x960
1280x1024
1360x768
1400x1050
1600x1200
1680x1050
1920x1200
WALL FUNCTIONS
Remove from Wall
Receiver (RX)
Preset:
Preset #1

- All Displays
  All

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  11
- Preset #2
  12
- Preset #3
  13
- Preset #4
  14
- Preset #5
  15
- Preset #6
  16
- Preset #7
  17
- Preset #8
  18
- Preset #9
  19

Classroom 1
3840x2160 60Hz RGB,8Bit
192.168.1.100-Genlock
SET VIDEO MODE
Genlock
Genlock Scaling
Fast Switch Full Screen
SET VIDEO
Leave Video Channel
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Video Formats
HD720P
HD1080P
4K UHD 2160P
Cinema Formats
4K Cinema 4096x2160
Graphics Formats
1024x768P
1280x768
1280x960
1280x1024
1360x768
1400x1050
1600x1200
1680x1050
1920x1200
Set Framebuffer Mode
Keep Aspect Ratio
Stretch to Fit
Crop to Fit
Video Formats
HD 720P 50Hz
HD 720P 60Hz
HD 1080P 50Hz
HD 1080P 60Hz
4K UHD 2160P 25Hz
4K UHD 2160P 30Hz
4K UHD 2160P 50Hz
4K UHD 2160P 60Hz
Cinema Formats
4K Cinema 4096x2160 24Hz
4K Cinema 4096x2160 30Hz
4K Cinema 4096x2160 60Hz
Video Formats
1024x768 60Hz
1280x768 60Hz
1280x960 60Hz
1280x1024 60Hz
1360x768 60Hz
1400x1050 60Hz
1600x1200 60Hz
1680x1050 60Hz
1920x1200 60Hz
SET VIDEO MODE
Start Video
Stop Video
Stop and Free Multicast address
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Receiver (RX)
Preset:
Preset #1

- All Displays

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  21
- Preset #2
  22
- Preset #3
  23
- Preset #4
  24
- Preset #5
  25
- Preset #6
  26
- Preset #7
  27
- Preset #8
  28
- Preset #9
  29

SET AUDIO
Leave HDMI Audio
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
SET AUDIO
Start HDMI Audio
Stop HDMI Audio
Stop and Free Multicast address
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Receiver (RX)
Preset:
Preset #1

- All Displays

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  31
- Preset #2
  32
- Preset #3
  33
- Preset #4
  34
- Preset #5
  35
- Preset #6
  36
- Preset #7
  37
- Preset #8
  38
- Preset #9
  39

SET AUDIO
Leave Analog Audio
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Factory Reset
Clean Settings
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
SET AUDIO
Start Analog Audio
Stop Analog Audio
Stop and Free Multicast address
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Receiver (RX)
Preset:
Preset #1

- All Displays
  All

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  41
- Preset #2
  42
- Preset #3
  43
- Preset #4
  44
- Preset #5
  45
- Preset #6
  46
- Preset #7
  47
- Preset #8
  48
- Preset #9
  49

DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
SET RS232
Stop RS232
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
Receiver (RX)
Preset:
Preset #1

- All Displays
  All

Transmitter (TX)
Groups:
Default

PRESET OPTIONS
Rename
Clear Preset
Save Preset
Recall Preset
Y N
GROUP OPTIONS
Rename
Delete Group
Y N

- Preset #1
  51
- Preset #2
  52
- Preset #3
  53
- Preset #4
  54
- Preset #5
  55
- Preset #6
  56
- Preset #7
  57
- Preset #8
  58
- Preset #9
  59

DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
SET INFRARED
Stop INFRARED
DEVICE OPTIONS
Settings
Send / Receive RS232
Send / Receive IR
Clean Settings
Factory Reset
Reboot
Remove from Group
Pin to this Position
Setting Backup
Setting Restore
All Devices

SET FIRMWARE UPDATE
Update
Backup and Restore
Backup
Name:
Save to:
Browse
Write Backup
Restore
Backup File:
Browse
Restore Backup
Security
Security
User Name:
admin
Old Password:
New Password:
Confirm Password:
Save
System Logs
Type Date & Time Event ID User Details

Save to ...
Clear Log
Video Routing Table
Hostname
Transmitter (TX) Receiver (RX)

- Hostname
- IP
- MAC

HDMI Audio Routing Table
Hostname
Transmitter (TX) Receiver (RX)

- Hostname
- IP
- MAC

Analog Audio Routing Table
Hostname
Transmitter (TX) Receiver (RX)

- Hostname
- IP
- MAC

RS232 Routing Table
Hostname
Transmitter (TX) Receiver (RX)

- Hostname
- IP
- MAC

Infrared Routing Table
Hostname
Transmitter (TX) Receiver (RX)

- Hostname
- IP
- MAC

Decoder XXX Configuration

- Analog Audio Output
- HDMI Audio Output
- Display EDID
- Network Setting
- RS232

SAVE
Analog Audio Output:
HDMI Audio(Downmix)
Analog Audio
HDMI Audio Output:
HDMI Audio(from HDMI Video in Genlock)
Analog Audio
HDMI Audio(Stereo Downmix)
HDMI Audio(All Available Channels)
Display EDID:
Save
Network Settings:
Hostname:
IP Mode:
IP Address:
Subnet Mask:
Default Gateway:
RS232:
Baud Rate:
Data Bit:
Stop Bit:
Parity:
OK
Encoder XXX Configuration

- Input
- Device EDID
- Network Setting
- RS232

SAVE
Input:
HDCP Support:
HDCP 2.2 Support:
Device EDID:
Load from File Save to Device
Network Settings:
Hostname:
IP Mode:
IP Address:
Subnet Mask:
Default Gateway:
RS232:
Baud Rate:
Data Bit:
Stop Bit:
Parity:
OK
Send / Receive RS-232 Data

- RS-232

Device
SEND
CLEAR
Send / Receive Infrared Data

- Infrared

Device
SEND
CLEAR
Clean Setting
Analog Audio Output
HDMI Audio Output
Network Setting
RS232
Set Video Genlock
HDCP Setting
Network Setting
RS232
YES NO
Device Setting Restore
YES NO
Stop and Free Multicast address
Are you sure?
YES NO
Factory Reset
Reset Device Now?
YES NO
Reboot Device
Reboot Device Now?
YES NO
Preset Save&Recall
Preset Save or Recall?
Save Recall
Delect Preset
Are you sure you want to delect: Preset #1
YES NO
Backup
Writing Backup File...
Backup Created Successfully!
Restore
Restoring...
Successfully Restored!
Error
Unable to connect to Server!
OK
Select File
OK
Edit
YES NO
Clear Preset Now?
YES NO
Save Preset Now?
YES NO
Recall Preset Now?
YES NO
Error
OK
Success
OK